(module LED_MEIHUA_MHPA1515RGBDT (layer F.Cu) (tedit 60EB0C32)
  (attr smd)
  (fp_text reference REF** (at 0 1.75) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value LED_MEIHUA_MHPA1515RGBDT (at 0 -1.75) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1 1) (end -1 -1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1 1) (end -1 1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1 -1) (end 1 1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1 -1) (end 1 -1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.8 0.75) (end -0.8 0.75) (layer F.Fab) (width 0.1))
  (fp_line (start -0.8 0.75) (end -0.8 -0.45) (layer F.Fab) (width 0.1))
  (fp_line (start -0.5 -0.75) (end 0.8 -0.75) (layer F.Fab) (width 0.1))
  (fp_line (start 0.8 -0.75) (end 0.8 0.75) (layer F.Fab) (width 0.1))
  (fp_line (start -0.8 -0.45) (end -0.5 -0.75) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.3 0.3) (thickness 0.05)))
  )
  (pad 1 smd rect (at -0.65 -0.4 180) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.65 -0.4 180) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0.65 0.4 180) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -0.65 0.4 180) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask))
)
