(module USB_A_Plug_PCB (layer F.Cu) (tedit 5F8DF2F0)
  (attr virtual)
  (fp_text reference REF** (at 0 10) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value USB_A_Plug_PCB (at 0 -1) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -6 11.75) (end -6 0) (layer Dwgs.User) (width 0.12))
  (fp_line (start -6 0) (end 6 0) (layer Dwgs.User) (width 0.12))
  (fp_line (start 6 0) (end 6 11.75) (layer Dwgs.User) (width 0.12))
  (pad 1 connect rect (at -3.5 4.945) (size 1 7.41) (layers F.Cu F.Mask))
  (pad 2 connect rect (at -1 5.445) (size 1 6.41) (layers F.Cu F.Mask))
  (pad 3 connect rect (at 1 5.445) (size 1 6.41) (layers F.Cu F.Mask))
  (pad 4 connect rect (at 3.5 4.945) (size 1 7.41) (layers F.Cu F.Mask))
  (pad 5 connect rect (at 0 4.575) (size 11 8.15) (layers B.Cu B.Mask))
)
