(footprint "Fader_Alps_RSx0N11M9A0x" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -12 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 8ede433a-4886-4b3b-b49c-066b9ed11afc)
  )
  (fp_text value "Fader_Alps_RSx0N11M9A0x" (at 0 138 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c912e07d-e795-495a-98b9-c52802efbe57)
  )
  (fp_text user "center of 60mm fader" (at 0 42.5 unlocked) (layer "Cmts.User")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 551369ec-f3e4-4842-b4b5-4614ce0e3407)
  )
  (fp_text user "center of 100mm fader" (at 0 62.5 unlocked) (layer "Cmts.User")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fa175549-9182-4073-809a-37e79b5f4bb9)
  )
  (fp_line (start -9.06 -10.41) (end -9.06 7.06) (layer "F.SilkS") (width 0.12) (tstamp 86724d71-3124-48ee-983e-3d857047c156))
  (fp_line (start -9.06 -10.41) (end 9.06 -10.41) (layer "F.SilkS") (width 0.12) (tstamp e170d7dc-96c1-4408-92db-8bbeb8438bca))
  (fp_line (start 9.06 -10.41) (end 9.06 7.06) (layer "F.SilkS") (width 0.12) (tstamp fd7af22d-dbc2-4c54-b0dd-0ee8c4b7610e))
  (fp_line (start -2 63.65) (end 2 63.65) (layer "Dwgs.User") (width 0.15) (tstamp 2ba9c327-c73b-4594-bc09-f8ebda4f1f8f))
  (fp_line (start -2 43.65) (end 2 43.65) (layer "Dwgs.User") (width 0.15) (tstamp a7e6cfc8-67d9-4726-9e05-9aa0e3bf7f9a))
  (fp_line (start -10 137.15) (end -10 -11.35) (layer "F.CrtYd") (width 0.05) (tstamp 0e79e179-2f69-473f-9d03-390fc0ff8435))
  (fp_line (start -10 -11.35) (end 10 -11.35) (layer "F.CrtYd") (width 0.05) (tstamp 7016f567-d1b0-4b2c-9f53-ade1586bc13b))
  (fp_line (start 10 137.15) (end -10 137.15) (layer "F.CrtYd") (width 0.05) (tstamp b41b33e2-7c12-482a-a5d1-03dd5daeff34))
  (fp_line (start 10 -11.35) (end 10 137.15) (layer "F.CrtYd") (width 0.05) (tstamp d0300b49-951b-46be-91f9-e9e8fca6ec7d))
  (fp_line (start -9 136.15) (end 9 136.15) (layer "F.Fab") (width 0.1) (tstamp 0a219dfe-13d8-4164-8413-ec98763b28f5))
  (fp_line (start -9 -10.35) (end -9 136.15) (layer "F.Fab") (width 0.1) (tstamp dc945bed-1257-4616-b513-4004d5fe238f))
  (fp_line (start -9 -10.35) (end 9 -10.35) (layer "F.Fab") (width 0.1) (tstamp e2eff81b-ec91-4f55-a825-0194c65ac572))
  (fp_line (start 9 -10.35) (end 9 136.15) (layer "F.Fab") (width 0.1) (tstamp ea25bdf0-16b5-4182-8636-5ffa8b84bc93))
  (pad "1" thru_hole circle (at 5.625 0) (size 2.3 2.3) (drill 1.5) (layers *.Cu *.Mask) (tstamp a86f9212-2656-4224-bbeb-977eebae6e55))
  (pad "2" thru_hole circle (at 1.875 0) (size 2.3 2.3) (drill 1.5) (layers *.Cu *.Mask) (tstamp 3acc54b0-c496-4d5d-93c0-039e09ba19fe))
  (pad "3" thru_hole circle (at -1.875 0) (size 2.3 2.3) (drill 1.5) (layers *.Cu *.Mask) (tstamp 983f04ba-d169-4bc6-891f-ffb6dfc68dff))
  (pad "4" thru_hole circle (at -5.625 0) (size 2.3 2.3) (drill 1.5) (layers *.Cu *.Mask) (tstamp 916f29fd-6baa-44c4-8146-a82ced5cdecb))
  (pad "MP" thru_hole circle (at 5.625 7) (size 2.8 2.8) (drill 2) (layers *.Cu *.Mask) (tstamp 194d17c1-d841-42db-9bbe-3a4cc6d183b4))
  (pad "MP" thru_hole circle (at 0 5.75) (size 2.8 2.8) (drill 2) (layers *.Cu *.Mask) (tstamp 2b8f2f01-b03d-4e71-aa45-c1f810fab011))
  (pad "MP" thru_hole circle (at -5.625 7) (size 2.8 2.8) (drill 2) (layers *.Cu *.Mask) (tstamp 53cda325-edb5-428d-adda-8c226e230fed))
)
