(footprint "Pad_1x01_SMD_2x5mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at 0 -4 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7bd1c578-28b8-48d9-a97f-a14a10423bcb)
  )
  (fp_text value "Pad_1x01_SMD_2x5mm" (at 0 4 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 132718d1-8d60-4e1a-8257-39853db659f3)
  )
  (pad "1" smd roundrect (at 0 0) (size 2 5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp ef2899f2-bbaa-4f1d-a89d-bbf5921b4a22))
)
