(kicad_pcb (version 20221018) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/")
    )
  )

  (net 0 "")
  (net 1 "+3V3")
  (net 2 "GND")
  (net 3 "/SDA")
  (net 4 "/SCL")
  (net 5 "unconnected-(J1-MountPin-PadMP)")
  (net 6 "Net-(U1-ADD0)")
  (net 7 "unconnected-(U1-ALERT-Pad3)")

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tstamp 16e6f23e-c166-44a1-9f32-b12460fe9c52)
    (at 144.65 104.325)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "temperature-sensor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (path "/078ee903-1990-41a6-8626-c6ea7f474166")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.16) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 711f3850-db44-4228-804e-0d6e651cce1e)
    )
    (fp_text value "100n" (at 0 1.16) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 84ceb97f-6a0a-4ce2-87b7-5654aa441581)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.25 0.25) (thickness 0.04)))
      (tstamp 5db57d7a-ff02-407b-8cd9-177bb5be90df)
    )
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7b888fc7-57f3-459f-8e30-6d2d7bcc2b90))
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7c96e367-1d1a-4822-afaf-4d8441188fd8))
    (fp_line (start -0.91 -0.46) (end 0.91 -0.46)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 62635a13-c7ff-427d-b836-e9575812eb22))
    (fp_line (start -0.91 0.46) (end -0.91 -0.46)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9855a7b6-452a-4468-b0e6-201d32bcfe6b))
    (fp_line (start 0.91 -0.46) (end 0.91 0.46)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 20d072fd-e5c5-4cf0-a27a-b3a99b1ade62))
    (fp_line (start 0.91 0.46) (end -0.91 0.46)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 247c159a-2c7b-4687-8ba1-5ba292e5a30b))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fc6da632-384e-42e6-989d-e25a93d04459))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 801f6b56-7913-4530-aea2-5e9147b459c4))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp acda7cf8-ec02-46a1-a4d2-a656da2a2395))
    (fp_line (start 0.5 0.25) (end -0.5 0.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp eaf2d304-4061-4dec-8b3a-eb32444e9f17))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive") (tstamp 628462e9-301a-4c36-8a81-eb76e1cf06d5))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 70db9ca5-194f-469c-b8dc-fc64485a13ca))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tstamp 49d08e51-f9bb-455a-8286-dfaae68be6a7)
    (at 143.33 105.255)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "temperature-sensor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (path "/243a6e74-f085-4816-ab87-58f0641cc5ac")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.17) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0508b033-2ab9-4f40-8dc2-121e1594fbdd)
    )
    (fp_text value "DNP" (at 0 1.17) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b676f79d-ae4d-4e77-a0cc-c5ddb47439c2)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.26 0.26) (thickness 0.04)))
      (tstamp 07f9a1b9-9a9b-475a-8097-c8e2f0412437)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 815a8fa3-b36e-4668-abea-f25084eda42b))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 33985cfd-6db8-4416-8800-d493b1740ad4))
    (fp_line (start -0.93 -0.47) (end 0.93 -0.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0921c2ce-30ba-4f61-84ae-43ec5ea2f3ff))
    (fp_line (start -0.93 0.47) (end -0.93 -0.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b5970c69-7a6f-4a08-9508-203ddafb8da4))
    (fp_line (start 0.93 -0.47) (end 0.93 0.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a23fd895-19cd-487d-b804-c1a867f818b5))
    (fp_line (start 0.93 0.47) (end -0.93 0.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c81f0166-88bd-4b4f-bee0-140d7acddd45))
    (fp_line (start -0.525 -0.27) (end 0.525 -0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 466e2cf5-da1c-4938-9e15-b3a0745dc161))
    (fp_line (start -0.525 0.27) (end -0.525 -0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ff93a175-afcd-4efc-aef2-5b12535303cd))
    (fp_line (start 0.525 -0.27) (end 0.525 0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4bfaaef3-0327-44e7-85fa-523d2dac30e3))
    (fp_line (start 0.525 0.27) (end -0.525 0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 244cf56c-54a2-4c20-b2e2-e2f6c84d62f0))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive") (tstamp 354422bb-a0d4-43e8-8bf1-2ef44261fa4b))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(U1-ADD0)") (pintype "passive") (tstamp 2fba87c9-22c8-4b10-8aca-c656b6515cb7))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "fosmometer:Jushuo_AFC01-S04FCx-00_1x04-1MP_P0.50mm_Horizontal" (layer "F.Cu")
    (tstamp 6982d3c3-1a20-430c-ab78-832a97a518f0)
    (at 149.595 102.34 90)
    (property "Sheetfile" "temperature-sensor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (path "/c28e1552-a625-429f-9d08-fccc8508897b")
    (attr smd)
    (fp_text reference "J1" (at 0 -5 90 unlocked) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dc0e05ec-05c3-49f1-9f88-47827c4b6d68)
    )
    (fp_text value "I2C" (at 0 4 90 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fb1f7b1c-0c2a-420f-a7c1-8b20228a941d)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.12)))
      (tstamp 3cf99c11-9d41-471c-89a7-ddcfc7f994d4)
    )
    (fp_line (start -3.31 -2.785) (end -1.11 -2.785)
      (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 009ae15f-b3ce-438f-8d3d-b9809c1fa3da))
    (fp_line (start -3.31 -1.355) (end -3.31 -2.785)
      (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 4bfc7685-f792-410c-b8f0-b1a844c09ca6))
    (fp_line (start -3.31 2.675) (end -3.31 0.665)
      (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 6542b42c-61a3-4ab7-bfaa-1bea772e3e21))
    (fp_line (start -1.11 -2.785) (end -1.11 -3.675)
      (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 0276dc0d-21d3-4bf0-ab52-d2042a280492))
    (fp_line (start 1.11 -2.785) (end 3.31 -2.785)
      (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 09b96e0b-3a34-4adf-a3a3-90d53426a12f))
    (fp_line (start 3.31 -1.355) (end 3.31 -2.785)
      (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 6f05c2f9-eb50-46b2-99e7-a23acdba82aa))
    (fp_line (start 3.31 2.675) (end 3.31 0.665)
      (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp a83f7fe9-71a5-4abb-91dd-e3cb0e8da9e1))
    (fp_line (start -3.7 -3.175) (end -1.4 -3.175)
      (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3c1ddaa2-9750-4464-9bc0-397c4ea6dcff))
    (fp_line (start -3.7 3.175) (end -3.7 -3.175)
      (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7a4434c1-733c-4acb-bf16-b044be9e3e6d))
    (fp_line (start -1.4 -4.175) (end 1.4 -4.175)
      (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6097e3b5-5385-4b4e-ad7e-a5494538ed87))
    (fp_line (start -1.4 -3.175) (end -1.4 -4.175)
      (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 91d25657-a651-44a5-b97e-8bb6d5e3fb9a))
    (fp_line (start 1.4 -4.175) (end 1.4 -3.175)
      (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 944a6ad3-7309-423d-9886-cf9d70d343bd))
    (fp_line (start 1.4 -3.175) (end 3.7 -3.175)
      (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3ea4225a-6329-49cc-9800-35c7b7f403c0))
    (fp_line (start 3.7 -3.175) (end 3.7 3.175)
      (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6f811a90-f2dd-41af-9c83-e40aa02da4ae))
    (fp_line (start 3.7 3.175) (end -3.7 3.175)
      (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 309869c2-5761-445a-a57e-7d4da83fd3d3))
    (fp_line (start -3.2 -2.675) (end 3.2 -2.675)
      (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 65107b58-14e5-4a45-8da1-fb28e27403e3))
    (fp_line (start -3.2 2.675) (end -3.2 -2.675)
      (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 087d0d0d-45dc-4537-9b64-46f9f91a4c1f))
    (fp_line (start 3.2 -2.675) (end 3.2 2.675)
      (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 7a8ed5bb-f1d1-4b1b-a9d6-8166f62f37a2))
    (fp_line (start 3.2 2.675) (end -3.2 2.675)
      (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 37edef19-b753-4bf5-8c94-ca4aae410f6a))
    (pad "1" smd roundrect (at -0.75 -3.025 90) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45) (tstamp 78988bc2-dfdf-4aff-8fa8-d1394833c099))
    (pad "2" smd roundrect (at -0.25 -3.025 90) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/SDA") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45) (tstamp 238d6115-de55-46c4-84c4-187772a5c8af))
    (pad "3" smd roundrect (at 0.25 -3.025 90) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/SCL") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45) (tstamp 40fb8046-ba36-460a-bbba-d3b921ed9763))
    (pad "4" smd roundrect (at 0.75 -3.025 90) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45) (tstamp 7ea98cd6-76c1-4608-8144-929c3aa86f43))
    (pad "MP" smd rect (at -2.45 -0.345 90) (size 2 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "unconnected-(J1-MountPin-PadMP)") (pinfunction "MountPin") (pintype "passive+no_connect") (thermal_bridge_angle 45) (tstamp a628e2b9-9bad-437c-98d3-4464cf6d7e75))
    (pad "MP" smd rect (at 2.45 -0.345 90) (size 2 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "unconnected-(J1-MountPin-PadMP)") (pinfunction "MountPin") (pintype "passive+no_connect") (thermal_bridge_angle 45) (tstamp 0d085d89-f840-47a6-93d2-f9ebb95b3b62))
  )

  (footprint "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm" (layer "F.Cu")
    (tstamp 90a22642-5d84-479c-a22f-80ca8731ef4d)
    (at 144.17 102.34 -90)
    (descr "WSON, 6 Pin (http://www.ti.com/lit/ds/symlink/tps61040.pdf#page=35), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "WSON NoLead")
    (property "Sheetfile" "temperature-sensor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Digital Temperature Sensor with I2C/SMBus Interface, 16 bits, +/-0.3° C, one-shot conversion, alert, nist traceable, EEPROM, WSON")
    (property "ki_keywords" "digital temperature sensor i2c smbus nist")
    (path "/151d4f42-fac5-411b-a661-f2a018008291")
    (attr smd)
    (fp_text reference "U1" (at 0 -1.95 90) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8ba9374e-5c7b-4256-b9eb-5f42a98740b8)
    )
    (fp_text value "TMP117xxDRV" (at 0 1.95 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8ee1f94c-db1b-46de-86db-d8757bee4983)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 92874e3b-7c5e-4f50-83e3-364e2d364beb)
    )
    (fp_line (start -1 1.11) (end 1 1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dd3a69b1-4539-412a-9b79-44da640ab2ab))
    (fp_line (start 0 -1.11) (end 1 -1.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a3acb182-87da-4156-9ee2-fff541daef6d))
    (fp_line (start -1.32 -1.25) (end -1.32 1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fe247a6a-6b8f-4a50-83bc-6014c7020f0c))
    (fp_line (start -1.32 1.25) (end 1.32 1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f7e9df37-f197-4922-bed0-546072f3029f))
    (fp_line (start 1.32 -1.25) (end -1.32 -1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f6676733-174e-4371-b184-ac3020b36695))
    (fp_line (start 1.32 1.25) (end 1.32 -1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b7359572-4d3b-401a-9e86-0955fefc7d34))
    (fp_line (start -1 -0.5) (end -0.5 -1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 42ed2ba9-7479-49eb-a524-802460033dbc))
    (fp_line (start -1 1) (end -1 -0.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 56ffc834-568d-48cb-8661-a71dbb701877))
    (fp_line (start -0.5 -1) (end 1 -1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0d79656a-2659-4efe-a1a9-05f18df18151))
    (fp_line (start 1 -1) (end 1 1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4b91c8ab-0e54-40fa-99fa-8dec43c49899))
    (fp_line (start 1 1) (end -1 1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6baba10c-1cbb-47ed-b833-2c4da550fdb4))
    (pad "" smd roundrect (at 0 -0.4 270) (size 0.81 0.64) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp ee4c5d87-39e3-4caf-bc5d-212269603e51))
    (pad "" smd roundrect (at 0 0.4 270) (size 0.81 0.64) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 597d7d23-8913-40e1-882a-eb28743cea19))
    (pad "1" smd roundrect (at -0.8875 -0.65 270) (size 0.375 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/SCL") (pinfunction "SCL") (pintype "input") (tstamp fd6097a0-1a38-4ef1-adc7-a142588179e6))
    (pad "2" smd roundrect (at -0.8875 0 270) (size 0.375 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp eadf306e-6730-4527-82c8-13fed3c8aa19))
    (pad "3" smd roundrect (at -0.8875 0.65 270) (size 0.375 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "unconnected-(U1-ALERT-Pad3)") (pinfunction "ALERT") (pintype "open_collector+no_connect") (tstamp 61dea7d3-d8c1-4e69-b47d-d752b103117d))
    (pad "4" smd roundrect (at 0.8875 0.65 270) (size 0.375 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(U1-ADD0)") (pinfunction "ADD0") (pintype "input") (tstamp 48d77c1f-0ac7-4452-9c83-e2544c7cdc1d))
    (pad "5" smd roundrect (at 0.8875 0 270) (size 0.375 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "V+") (pintype "power_in") (tstamp 00e961e4-2e9c-4a49-b057-37fcae4a1bb4))
    (pad "6" smd roundrect (at 0.8875 -0.65 270) (size 0.375 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/SDA") (pinfunction "SDA") (pintype "bidirectional") (tstamp 906ecf97-b54f-4075-844f-3ca7f01403e3))
    (pad "7" smd rect (at 0 0 270) (size 1 1.6) (layers "F.Cu" "F.Mask") (tstamp 4ccfcccf-c95d-4b2d-9c19-44f83410666d))
    (model "${KICAD6_3DMODEL_DIR}/Package_SON.3dshapes/WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tstamp b3f59e70-89bf-40d7-bffa-a0c514667d20)
    (at 145.49 105.255 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "temperature-sensor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (path "/b12bdde3-4ba8-452b-95d0-21958345a4f0")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.17) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a9eb814c-cba4-4165-8c9a-5d58f8050532)
    )
    (fp_text value "DNP" (at 0 1.17) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0caa269d-0a64-47d1-ac29-58043d4e9cc3)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.26 0.26) (thickness 0.04)))
      (tstamp aa848e15-b3a0-42e0-b7d9-c0e0e69552b4)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 94ea9b3d-86d3-40c0-b550-7b057dc37a82))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1dac5654-d6db-4a1d-ba9d-a85bb1da33ff))
    (fp_line (start -0.93 -0.47) (end 0.93 -0.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f1a937ee-c23b-4e87-b230-023a30f28aed))
    (fp_line (start -0.93 0.47) (end -0.93 -0.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4f92e0b9-4b96-4afc-ab47-ec786d87c5c0))
    (fp_line (start 0.93 -0.47) (end 0.93 0.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 985df32a-29ab-4d77-a9ff-e0b11821f4f7))
    (fp_line (start 0.93 0.47) (end -0.93 0.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a1231840-5824-44dd-8645-dddd9df11511))
    (fp_line (start -0.525 -0.27) (end 0.525 -0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 063abde1-13e7-4516-adf7-73739636bf4c))
    (fp_line (start -0.525 0.27) (end -0.525 -0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3e65c041-9232-4528-ba61-b9082095bdf7))
    (fp_line (start 0.525 -0.27) (end 0.525 0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp adddc350-a272-4615-b3ff-e0999fd9ef17))
    (fp_line (start 0.525 0.27) (end -0.525 0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ff6fe5b4-2a03-4059-a243-2763bff66ba7))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/SDA") (pintype "passive") (tstamp 4b83b047-b4ad-451a-bf6d-1280ecac5dc6))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(U1-ADD0)") (pintype "passive") (tstamp 3d6736e8-b2e3-4e9b-89f0-88ad922ba3f4))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tstamp d992d106-2438-4c34-8528-19529887a382)
    (at 143.33 100.345 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "temperature-sensor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (path "/2471d8b2-a9b2-481f-837e-41a8cc4fc319")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.17) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 69df4b12-1503-408b-b5af-b238a1247168)
    )
    (fp_text value "DNP" (at 0 1.17) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 425567e2-c18b-49ea-806e-162a6ea22338)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.26 0.26) (thickness 0.04)))
      (tstamp b7352b16-2833-45e5-866e-897838f88f92)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2cfcdf69-f506-4c36-b7a6-2f95af6a1ab7))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 85e0aee0-4da1-484e-a44d-32f0a19c673d))
    (fp_line (start -0.93 -0.47) (end 0.93 -0.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a35504d2-b97c-4b52-a9bc-0b1d50c0f4ee))
    (fp_line (start -0.93 0.47) (end -0.93 -0.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1990c9d3-d339-444b-bec6-4106453c5225))
    (fp_line (start 0.93 -0.47) (end 0.93 0.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f4da766c-b825-49f3-933c-8a05d87705f5))
    (fp_line (start 0.93 0.47) (end -0.93 0.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 04c567e0-f4fc-4bb2-8b92-63fdcaf72c67))
    (fp_line (start -0.525 -0.27) (end 0.525 -0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2e3dd97e-5c65-475e-935d-e9e424da49ae))
    (fp_line (start -0.525 0.27) (end -0.525 -0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 80ae85ce-e4f9-46a1-9710-ef4ac0a02e42))
    (fp_line (start 0.525 -0.27) (end 0.525 0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e611ce9f-1759-4579-85b9-a8df1008e089))
    (fp_line (start 0.525 0.27) (end -0.525 0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c67fb021-76a7-4496-b341-a8516e7eedd8))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(U1-ADD0)") (pintype "passive") (tstamp 5293181c-f269-4af8-8138-b4ce01efe01f))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/SCL") (pintype "passive") (tstamp d0b5e36c-1218-4990-bee7-2b34d4babbd9))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tstamp fb90527e-5d67-4ca6-adab-d11f429d9e94)
    (at 145.49 100.345)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "temperature-sensor.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (path "/de580c43-f534-475a-80f4-a92d77752dc5")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.17) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ade83ea5-b884-4fa4-92b9-9fa914e421cd)
    )
    (fp_text value "0R" (at 0 1.17) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7ecf4989-fdcf-450a-b58c-ce07d5b2cc84)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.26 0.26) (thickness 0.04)))
      (tstamp f0e082ba-ebad-48c3-9807-c183ace45cf3)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b6748c08-885c-45e8-bf8e-5c5410f7bb03))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7a0649c6-7bdb-4bc5-8e23-420cf51b60bc))
    (fp_line (start -0.93 -0.47) (end 0.93 -0.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp df89e343-eacd-4ec0-872e-8967024ff4aa))
    (fp_line (start -0.93 0.47) (end -0.93 -0.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 367fc126-e538-446c-9624-d4eaeb3e53c3))
    (fp_line (start 0.93 -0.47) (end 0.93 0.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 32b0b83f-b289-462c-8485-0cbd1cefd41f))
    (fp_line (start 0.93 0.47) (end -0.93 0.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2a0c96d6-e9f7-4f73-881e-3c3798ef0aff))
    (fp_line (start -0.525 -0.27) (end 0.525 -0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2bddde54-aca8-4dd7-8ae1-32d63066bb16))
    (fp_line (start -0.525 0.27) (end -0.525 -0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp eb358eb1-b894-487b-9d02-6328a51f61bd))
    (fp_line (start 0.525 -0.27) (end 0.525 0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7c1b536b-244e-4c88-9475-062a3fc6d8fd))
    (fp_line (start 0.525 0.27) (end -0.525 0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7938b9eb-2531-4b28-9bfd-17aa7f60b32a))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(U1-ADD0)") (pintype "passive") (tstamp 6436bd43-9299-40aa-a4a3-488b88271c1c))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp be39cef2-bf58-484c-babd-bfb86f53911d))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_poly
    (pts
      (xy 142.97 101.84)
      (xy 144.97 101.84)
      (xy 144.97 102.84)
      (xy 142.97 102.84)
      (xy 141.97 103.84)
      (xy 138.97 103.84)
      (xy 138.97 100.84)
      (xy 141.97 100.84)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.Cu") (tstamp 73d92917-b996-422d-9343-4bf3a8a1436f))
  (gr_poly
    (pts
      (xy 142.97 101.84)
      (xy 142.97 102.84)
      (xy 141.97 103.84)
      (xy 138.97 103.84)
      (xy 138.97 100.84)
      (xy 141.97 100.84)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.Mask") (tstamp 2b9a4138-cdbc-4843-aee8-4879ec2fee12))
  (gr_arc (start 151.77 98.39) (mid 152.123553 98.536447) (end 152.27 98.89)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 139d7289-2c3b-4d38-821c-4f9247785348))
  (gr_line (start 152.27 98.89) (end 152.27 105.79)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 280ce04f-b304-4cca-9fbb-6431d369fd2e))
  (gr_arc (start 142.55 106.29) (mid 142.196447 106.143553) (end 142.05 105.79)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 2e9b687c-cbf2-442d-80db-0a4d92edbcfc))
  (gr_arc (start 152.27 105.79) (mid 152.123553 106.143553) (end 151.77 106.29)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 4fbed71d-20b7-430d-aa4d-ddd35c31fe97))
  (gr_line (start 142.55 106.29) (end 151.77 106.29)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 55507abf-f671-4d21-a54f-891bcfb183c3))
  (gr_line (start 138.97 104.04) (end 141.85 104.04)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 5f4565cd-c0e3-49aa-b417-dda2f9d81e9c))
  (gr_line (start 142.05 100.44) (end 142.05 98.89)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 5fc1a9be-303a-4f1d-91bd-f225372671bd))
  (gr_arc (start 138.77 100.84) (mid 138.828579 100.698579) (end 138.97 100.64)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 78f57801-d0bd-4a81-aa23-49a37ae8b3dd))
  (gr_line (start 142.05 104.24) (end 142.05 105.79)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 8551b996-12b9-4d7f-a121-db8054833cad))
  (gr_arc (start 141.85 104.04) (mid 141.991421 104.098579) (end 142.05 104.24)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 9ef3e1f8-1776-45fe-8304-911c13bc67cc))
  (gr_arc (start 138.97 104.04) (mid 138.828579 103.981421) (end 138.77 103.84)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp c70be04c-64f4-43a2-91bd-77621efb2956))
  (gr_line (start 138.77 100.84) (end 138.77 103.84)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp d3cf7d95-0738-44c6-83cc-be8858c5dbd7))
  (gr_line (start 142.55 98.39) (end 151.77 98.39)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp d9da579c-e320-4b70-82b2-94b66dd82489))
  (gr_arc (start 142.05 100.44) (mid 141.991421 100.581421) (end 141.85 100.64)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp e8decd87-1241-4694-86f9-a7389643f77d))
  (gr_arc (start 142.05 98.89) (mid 142.196447 98.536447) (end 142.55 98.39)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp f712c690-2d00-44b5-b090-c1c9f07998c5))
  (gr_line (start 141.85 100.64) (end 138.97 100.64)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp f7d4eed9-2577-4a9e-a199-04ae0eee9d6b))
  (gr_text "lujoga 2024" (at 151.77 104.29) (layer "B.SilkS") (tstamp 5adf14aa-4798-4c84-81a9-45c768368be7)
    (effects (font (size 0.8 0.8) (thickness 0.12)) (justify left bottom mirror))
  )
  (gr_text "temperature\nsensor v1" (at 151.77 98.89) (layer "B.SilkS") (tstamp 8e7cdeb1-eb86-4b03-bea6-a645d72663e4)
    (effects (font (size 1 1) (thickness 0.15)) (justify left top mirror))
  )
  (gr_text "1" (at 142.82 104.785) (layer "F.SilkS") (tstamp 44714ffb-5d38-4a8d-9ea1-2c1570c9e473)
    (effects (font (size 1 1) (thickness 0.15)) (justify bottom))
  )
  (gr_text "0" (at 145.49 99.9) (layer "F.SilkS") (tstamp c5c32e3c-5931-4360-a8cf-38d091945c15)
    (effects (font (size 1 1) (thickness 0.15)) (justify bottom))
  )
  (gr_text "2" (at 146 104.785) (layer "F.SilkS") (tstamp eacd329d-eaff-4d50-b13d-ad706e165802)
    (effects (font (size 1 1) (thickness 0.15)) (justify bottom))
  )
  (gr_text "3" (at 143.33 99.9) (layer "F.SilkS") (tstamp f5a76fda-af32-4bf4-a682-69beae4d868d)
    (effects (font (size 1 1) (thickness 0.15)) (justify bottom))
  )

  (segment (start 144.78 103.715) (end 144.17 104.325) (width 0.2) (layer "F.Cu") (net 1) (tstamp 3e3c3cbe-350e-4bfd-8dbf-7658030c627d))
  (segment (start 142.82 105.255) (end 143.75 104.325) (width 0.2) (layer "F.Cu") (net 1) (tstamp 56a1ac89-8cba-43a5-9f53-635d373c3320))
  (segment (start 144.17 103.2275) (end 144.17 104.325) (width 0.2) (layer "F.Cu") (net 1) (tstamp 656236e9-08e7-4e95-9913-cb682497a2ad))
  (segment (start 145.945 103.715) (end 144.78 103.715) (width 0.2) (layer "F.Cu") (net 1) (tstamp 6d14a47f-f8a9-4023-9cab-28461aaffcb1))
  (segment (start 143.75 104.325) (end 144.17 104.325) (width 0.2) (layer "F.Cu") (net 1) (tstamp 7b9ba393-e5a6-404e-ac83-efa20ca62f5d))
  (segment (start 146.57 103.09) (end 145.945 103.715) (width 0.2) (layer "F.Cu") (net 1) (tstamp b62a3fb1-2c20-4afb-b251-c19cefc09194))
  (segment (start 146 100.91) (end 145.945 100.965) (width 0.2) (layer "F.Cu") (net 2) (tstamp 41c0db2f-3c11-44b5-b358-590de5d6eb7e))
  (segment (start 144.470001 100.965) (end 144.17 101.265001) (width 0.2) (layer "F.Cu") (net 2) (tstamp 45422de5-531e-4245-94e3-2a398201b8fd))
  (segment (start 146.57 101.59) (end 146.82 101.34) (width 0.2) (layer "F.Cu") (net 2) (tstamp 4e4ead38-eb81-48f0-a99e-4c43f01bd8b5))
  (segment (start 144.17 101.265001) (end 144.17 101.4525) (width 0.2) (layer "F.Cu") (net 2) (tstamp 645b2bdd-def2-4ad9-80fe-f9a701f9dd3c))
  (segment (start 146.82 101.34) (end 147.94 101.34) (width 0.2) (layer "F.Cu") (net 2) (tstamp 6c552797-300c-47bd-82ef-086cc114735d))
  (segment (start 148.27 102.988529) (end 146.933529 104.325) (width 0.2) (layer "F.Cu") (net 2) (tstamp 6f638ca2-8286-45cd-8cd6-b50258d24bad))
  (segment (start 147.94 101.34) (end 148.27 101.67) (width 0.2) (layer "F.Cu") (net 2) (tstamp 805be5fb-5c47-43fb-b5f4-94714b32f622))
  (segment (start 146.57 101.59) (end 145.945 100.965) (width 0.2) (layer "F.Cu") (net 2) (tstamp 8e5c1edc-7650-4185-8c35-c014508c2088))
  (segment (start 146 100.345) (end 146 100.91) (width 0.2) (layer "F.Cu") (net 2) (tstamp a39eabe6-b1d0-4701-8544-9f01d7c97f2f))
  (segment (start 146.933529 104.325) (end 145.13 104.325) (width 0.2) (layer "F.Cu") (net 2) (tstamp e6dfdb76-ee7c-4bc8-a8e8-fa08435cdb0d))
  (segment (start 148.27 101.67) (end 148.27 102.988529) (width 0.2) (layer "F.Cu") (net 2) (tstamp e80335d4-8fa2-4ebe-8f34-0277b3c6e697))
  (segment (start 145.945 100.965) (end 144.470001 100.965) (width 0.2) (layer "F.Cu") (net 2) (tstamp f19a8c44-ce00-46e4-90d5-e419dc38975a))
  (segment (start 146.57 102.59) (end 145.82 102.59) (width 0.2) (layer "F.Cu") (net 3) (tstamp 00eb7405-9c00-4a7e-bfa4-2bffded715fb))
  (segment (start 145.1825 103.2275) (end 144.82 103.2275) (width 0.2) (layer "F.Cu") (net 3) (tstamp 42f6bd41-3328-41fa-813a-5cc678910309))
  (segment (start 146 105.255) (end 146.57 105.255) (width 0.2) (layer "F.Cu") (net 3) (tstamp 56203232-1a0e-4c2c-a141-9671e4b028db))
  (segment (start 147.52 102.59) (end 147.67 102.74) (width 0.2) (layer "F.Cu") (net 3) (tstamp 7ec76251-1b3f-4e7d-a844-83e25ae5ff2f))
  (segment (start 146.57 102.59) (end 147.52 102.59) (width 0.2) (layer "F.Cu") (net 3) (tstamp 8f519bf4-8bf6-4315-b687-b914e510f66d))
  (segment (start 145.82 102.59) (end 145.1825 103.2275) (width 0.2) (layer "F.Cu") (net 3) (tstamp a9972bd8-3ae2-4345-83e7-d87606f4b0b6))
  (via (at 146.57 105.255) (size 0.6) (drill 0.4) (layers "F.Cu" "B.Cu") (net 3) (tstamp 72ed7816-e8b0-4574-b6e3-1369cb947284))
  (via (at 147.67 102.74) (size 0.6) (drill 0.4) (layers "F.Cu" "B.Cu") (net 3) (tstamp e3c812f1-8ba5-4805-a761-b8c9d044ef44))
  (segment (start 147.67 102.74) (end 147.67 104.155) (width 0.2) (layer "B.Cu") (net 3) (tstamp 8c646a3e-6287-4bf1-b025-cd21bb57fb2f))
  (segment (start 147.67 104.155) (end 146.57 105.255) (width 0.2) (layer "B.Cu") (net 3) (tstamp 99072e50-8df1-47d7-9f0c-05e480c8c805))
  (segment (start 145.82 102.09) (end 145.1825 101.4525) (width 0.2) (layer "F.Cu") (net 4) (tstamp 0fd16b9c-8402-4b67-af88-0724c90bae5d))
  (segment (start 146.57 102.09) (end 145.82 102.09) (width 0.2) (layer "F.Cu") (net 4) (tstamp 459b51f1-490e-46a4-b17e-daa8f0bd2f42))
  (segment (start 145.1825 101.4525) (end 144.82 101.4525) (width 0.2) (layer "F.Cu") (net 4) (tstamp 505a7928-6a3c-4a3e-a6e3-5287e105497e))
  (segment (start 147.52 102.09) (end 147.67 101.94) (width 0.2) (layer "F.Cu") (net 4) (tstamp 90609145-956c-4def-ae9e-869b50b67adc))
  (segment (start 146.57 102.09) (end 147.52 102.09) (width 0.2) (layer "F.Cu") (net 4) (tstamp 9ca19852-85e5-4d97-bd29-62c7bbba5011))
  (segment (start 142.82 99.725) (end 142.82 100.345) (width 0.2) (layer "F.Cu") (net 4) (tstamp b471e151-68d0-4999-91bb-e31f7be127b8))
  (via (at 147.67 101.94) (size 0.6) (drill 0.4) (layers "F.Cu" "B.Cu") (net 4) (tstamp 590e208a-7c53-4cd7-b79e-214f148e9633))
  (via (at 142.82 99.725) (size 0.6) (drill 0.4) (layers "F.Cu" "B.Cu") (net 4) (tstamp deff32b8-01af-4382-8bc5-e9fd47da9b39))
  (segment (start 147.67 101.94) (end 145.455 99.725) (width 0.2) (layer "B.Cu") (net 4) (tstamp d001ba2f-e826-4ffa-aeb3-fcaa05bdd0b1))
  (segment (start 145.455 99.725) (end 142.82 99.725) (width 0.2) (layer "B.Cu") (net 4) (tstamp f84e8d1e-ac05-4935-84b0-ce5775971c5b))
  (segment (start 144.41 100.345) (end 144.98 100.345) (width 0.2) (layer "F.Cu") (net 6) (tstamp 39b43ef4-bd79-4d4f-ade9-2e1bc3079c07))
  (segment (start 144.41 105.255) (end 144.98 105.255) (width 0.2) (layer "F.Cu") (net 6) (tstamp 41b04f5c-9c14-48ff-a1fe-c485f21e2caf))
  (segment (start 143.84 105.255) (end 144.41 105.255) (width 0.2) (layer "F.Cu") (net 6) (tstamp 432ce257-7c76-4c45-b54b-5491d5643a65))
  (segment (start 143.84 100.345) (end 144.41 100.345) (width 0.2) (layer "F.Cu") (net 6) (tstamp 555b3de9-ee5d-4c88-a6de-119e5668e7f2))
  (segment (start 143.52 103.2275) (end 143.52 103.715) (width 0.2) (layer "F.Cu") (net 6) (tstamp b3f44582-6282-4d8a-9c86-447c31d87f07))
  (via (at 143.52 103.715) (size 0.6) (drill 0.4) (layers "F.Cu" "B.Cu") (net 6) (tstamp 35ae6fe1-5a61-4222-bc28-b1d78d137fbb))
  (via (at 144.41 105.255) (size 0.6) (drill 0.4) (layers "F.Cu" "B.Cu") (net 6) (tstamp 39eb989c-fef2-4ce8-ba26-a9e92c21dabd))
  (via (at 144.41 100.345) (size 0.6) (drill 0.4) (layers "F.Cu" "B.Cu") (net 6) (tstamp 6b29b385-9d66-41c9-86e6-8364999e0838))
  (segment (start 143.52 104.365) (end 144.41 105.255) (width 0.2) (layer "B.Cu") (net 6) (tstamp 50c14d56-ecb6-4ade-a465-f7cdadab43b8))
  (segment (start 143.52 103.715) (end 143.52 104.365) (width 0.2) (layer "B.Cu") (net 6) (tstamp 571a81fa-8f27-4edd-967c-4c4c45136fb4))
  (segment (start 143.52 103.715) (end 143.52 101.235) (width 0.2) (layer "B.Cu") (net 6) (tstamp 8ddc0cc8-e186-41e8-9ea0-2225cf0f1304))
  (segment (start 143.52 101.235) (end 144.41 100.345) (width 0.2) (layer "B.Cu") (net 6) (tstamp fef9ac3b-54e6-4ff2-b4cf-6c772b513bd0))

)
