(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "CH32V003J4M6" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -13.97 -6.35 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Value" "CH32V003J4M6" (at -13.97 -8.89 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "Package_SO:SOP-8_3.9x4.9mm_P1.27mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.wch-ic.com/downloads/CH32V003DS0_PDF.html" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "CH32V003J4M6_0_0"
      (pin bidirectional line (at -15.24 3.81 0) (length 2.54)
        (name "PD6/URX" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 1.27 0) (length 2.54)
        (name "PA2/TICH2N" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 12.7 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 3.81 180) (length 2.54)
        (name "PC1/SDA" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 1.27 180) (length 2.54)
        (name "PC2/SCL" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -1.27 180) (length 2.54)
        (name "PC4/TICH4" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -3.81 180) (length 2.54)
        (name "PD1/SWIO/PD5/UTX" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "CH32V003J4M6_1_1"
      (rectangle (start -12.7 10.16) (end 12.7 -10.16)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
  )
  (symbol "SY8201" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 13.97 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SY8201" (at 0 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-6" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheet.lcsc.com/lcsc/1810161442_Silergy-Corp-SY8201ABC_C108052.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SY8201_0_0"
      (pin passive line (at 8.89 7.62 180) (length 2.54)
        (name "BS" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 8.89 -7.62 180) (length 2.54)
        (name "FB" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -8.89 3.81 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 7.62 0) (length 2.54)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 8.89 0 180) (length 2.54)
        (name "LX" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "SY8201_1_1"
      (rectangle (start -6.35 10.16) (end 6.35 -10.16)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
  )
)
