(footprint "Jushuo_AFC01-S04FCx-00_1x04-1MP_P0.50mm_Horizontal" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 0a4dc1ca-3227-4c09-a5a4-30e4aa9a0a47)
  )
  (fp_text value "Jushuo_AFC01-S04FCx-00_1x04-1MP_P0.50mm_Horizontal" (at 0 4 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 595321ad-a150-4a5d-a1a8-ee5b3d2d0f84)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    (tstamp e5824777-ccde-463f-9604-3e8e6cacf6ae)
  )
  (fp_line (start -3.31 -2.785) (end -1.11 -2.785)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 50ac20ce-437f-4369-bfc4-f7418e44240c))
  (fp_line (start -3.31 -1.355) (end -3.31 -2.785)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 6b9fc076-3b61-436d-8abe-a5e8dfb3128e))
  (fp_line (start -3.31 2.675) (end -3.31 0.665)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 5e419a27-5526-4bd2-b3ac-7c4022a042f2))
  (fp_line (start -1.11 -2.785) (end -1.11 -3.675)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 14068898-a3be-4389-bbf5-53d74d5293c9))
  (fp_line (start 1.11 -2.785) (end 3.31 -2.785)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 9b8d19c4-2c3b-462f-ad8d-9195e564d9ba))
  (fp_line (start 3.31 -1.355) (end 3.31 -2.785)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 166df502-f473-43ba-a340-877979a4cbd8))
  (fp_line (start 3.31 2.675) (end 3.31 0.665)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 6e9fb18f-449d-4d4f-80d5-d9532298fa78))
  (fp_line (start -3.7 -3.175) (end -1.4 -3.175)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 702b127e-1778-4ca2-9f7b-5f710a9ae30c))
  (fp_line (start -3.7 3.175) (end -3.7 -3.175)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7e99eb88-4c78-446b-bf8c-cf32a48e8765))
  (fp_line (start -1.4 -4.175) (end 1.4 -4.175)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp bd1dc6e3-7dcc-47eb-80a9-bf0b5c407b73))
  (fp_line (start -1.4 -3.175) (end -1.4 -4.175)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 93184e3d-7a9c-45ac-9275-b255e8e9764c))
  (fp_line (start 1.4 -4.175) (end 1.4 -3.175)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9da501d4-a7b8-4b24-97f6-20454c0ffd38))
  (fp_line (start 1.4 -3.175) (end 3.7 -3.175)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c320b22e-654d-47f0-92f4-37fffb1541dc))
  (fp_line (start 3.7 -3.175) (end 3.7 3.175)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9b7a1cb6-e5e1-40ba-bf03-56750ee384b9))
  (fp_line (start 3.7 3.175) (end -3.7 3.175)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp be45539c-b091-4b3e-b896-2eb1aabd5e5c))
  (fp_line (start -3.2 -2.675) (end 3.2 -2.675)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 266bae49-9d5c-4597-9fd3-aa1d0111c84d))
  (fp_line (start -3.2 2.675) (end -3.2 -2.675)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp d0cbd4b6-a59f-4556-b15a-d7d47a7e2626))
  (fp_line (start 3.2 -2.675) (end 3.2 2.675)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 208b69df-4ef5-446a-adf5-0fd462c7cf19))
  (fp_line (start 3.2 2.675) (end -3.2 2.675)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 1821c262-698d-4675-b620-9653634e7e37))
  (pad "1" smd roundrect (at -0.75 -3.025) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 7fb4ab58-820c-4fef-a9c7-ba79ce561e47))
  (pad "2" smd roundrect (at -0.25 -3.025) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 5725b7ce-9bb0-4952-bf23-1385ad63a963))
  (pad "3" smd roundrect (at 0.25 -3.025) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 8e39203e-22cb-4f4f-80e8-8211ae056a9a))
  (pad "4" smd roundrect (at 0.75 -3.025) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp d2cc08bf-6eec-47a1-8459-53c3816b8a7e))
  (pad "MP" smd rect (at -2.45 -0.345) (size 2 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 962ce400-7c45-426c-ae06-41e7dd005e31))
  (pad "MP" smd rect (at 2.45 -0.345) (size 2 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp c3513d95-c1b9-40fb-a55c-8778438d768c))
)
