(footprint "Fader_Alps_RSA0N11M9A0J"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -12 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "8ede433a-4886-4b3b-b49c-066b9ed11afc")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Fader_Alps_RSA0N11M9A0J"
		(at 0 138 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "c912e07d-e795-495a-98b9-c52802efbe57")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "8f2dd91c-64d0-43c9-9808-cfaa27f84b3d")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "3c61e9c4-bac3-4f1d-9998-1ab48bb8ab3c")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "39f078eb-f02e-47e2-8ed3-85fc4c148ecd")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -9.06 -10.41)
		(end -9.06 7.06)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "86724d71-3124-48ee-983e-3d857047c156")
	)
	(fp_line
		(start -9.06 -10.41)
		(end 9.06 -10.41)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e170d7dc-96c1-4408-92db-8bbeb8438bca")
	)
	(fp_line
		(start 9.06 -10.41)
		(end 9.06 7.06)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "fd7af22d-dbc2-4c54-b0dd-0ee8c4b7610e")
	)
	(fp_line
		(start -2 63.65)
		(end 2 63.65)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "Dwgs.User")
		(uuid "2ba9c327-c73b-4594-bc09-f8ebda4f1f8f")
	)
	(fp_line
		(start -10 -11.35)
		(end 10 -11.35)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7016f567-d1b0-4b2c-9f53-ade1586bc13b")
	)
	(fp_line
		(start -10 137.15)
		(end -10 -11.35)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "0e79e179-2f69-473f-9d03-390fc0ff8435")
	)
	(fp_line
		(start 10 -11.35)
		(end 10 137.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d0300b49-951b-46be-91f9-e9e8fca6ec7d")
	)
	(fp_line
		(start 10 137.15)
		(end -10 137.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b41b33e2-7c12-482a-a5d1-03dd5daeff34")
	)
	(fp_line
		(start -9 -10.35)
		(end -9 136.15)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "dc945bed-1257-4616-b513-4004d5fe238f")
	)
	(fp_line
		(start -9 -10.35)
		(end 9 -10.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e2eff81b-ec91-4f55-a825-0194c65ac572")
	)
	(fp_line
		(start -9 136.15)
		(end 9 136.15)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0a219dfe-13d8-4164-8413-ec98763b28f5")
	)
	(fp_line
		(start 9 -10.35)
		(end 9 136.15)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ea25bdf0-16b5-4182-8636-5ffa8b84bc93")
	)
	(fp_text user "center"
		(at 0 62.5 0)
		(unlocked yes)
		(layer "Cmts.User")
		(uuid "fa175549-9182-4073-809a-37e79b5f4bb9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 5.625 0)
		(size 2.3 2.3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a86f9212-2656-4224-bbeb-977eebae6e55")
	)
	(pad "2" thru_hole circle
		(at 1.875 0)
		(size 2.3 2.3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3acc54b0-c496-4d5d-93c0-039e09ba19fe")
	)
	(pad "3" thru_hole circle
		(at -1.875 0)
		(size 2.3 2.3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "983f04ba-d169-4bc6-891f-ffb6dfc68dff")
	)
	(pad "4" thru_hole circle
		(at -5.625 0)
		(size 2.3 2.3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "916f29fd-6baa-44c4-8146-a82ced5cdecb")
	)
	(pad "5" thru_hole circle
		(at 4 93.2)
		(size 2.3 2.3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f2d8d434-22b0-4246-bd40-14887c46133c")
	)
	(pad "6" thru_hole circle
		(at -4 93.2)
		(size 2.3 2.3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "72dbba10-b091-4708-a27d-9f2193c6a945")
	)
	(pad "MP" thru_hole circle
		(at -5.625 7)
		(size 2.8 2.8)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "53cda325-edb5-428d-adda-8c226e230fed")
	)
	(pad "MP" thru_hole circle
		(at 0 5.75)
		(size 2.8 2.8)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2b8f2f01-b03d-4e71-aa45-c1f810fab011")
	)
	(pad "MP" thru_hole circle
		(at 5.625 7)
		(size 2.8 2.8)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "194d17c1-d841-42db-9bbe-3a4cc6d183b4")
	)
	(model "${KIPRJMOD}/3d/RSA0N11M9A0J.STEP"
		(offset
			(xyz 0 -63.5 26)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 90)
		)
	)
)
