(footprint "Jushuo_AFC01-S04FCx-00_1x04-1MP_P0.50mm_Horizontal"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "0a4dc1ca-3227-4c09-a5a4-30e4aa9a0a47")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Jushuo_AFC01-S04FCx-00_1x04-1MP_P0.50mm_Horizontal"
		(at 0 4 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "595321ad-a150-4a5d-a1a8-ee5b3d2d0f84")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "0377cbe4-4dcf-4a0a-ae16-72cd4d9c9011")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "24375f52-5092-40e3-bf19-4dbe2a6aa412")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "9c50a82d-7ebd-46d4-baa6-5ce8ac102aca")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -3.31 -2.785)
		(end -1.11 -2.785)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "50ac20ce-437f-4369-bfc4-f7418e44240c")
	)
	(fp_line
		(start -3.31 -1.355)
		(end -3.31 -2.785)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "6b9fc076-3b61-436d-8abe-a5e8dfb3128e")
	)
	(fp_line
		(start -3.31 2.675)
		(end -3.31 0.665)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "5e419a27-5526-4bd2-b3ac-7c4022a042f2")
	)
	(fp_line
		(start -1.11 -2.785)
		(end -1.11 -3.675)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "14068898-a3be-4389-bbf5-53d74d5293c9")
	)
	(fp_line
		(start 1.11 -2.785)
		(end 3.31 -2.785)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "9b8d19c4-2c3b-462f-ad8d-9195e564d9ba")
	)
	(fp_line
		(start 3.31 -1.355)
		(end 3.31 -2.785)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "166df502-f473-43ba-a340-877979a4cbd8")
	)
	(fp_line
		(start 3.31 2.675)
		(end 3.31 0.665)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "6e9fb18f-449d-4d4f-80d5-d9532298fa78")
	)
	(fp_line
		(start -3.7 -3.175)
		(end -1.4 -3.175)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "702b127e-1778-4ca2-9f7b-5f710a9ae30c")
	)
	(fp_line
		(start -3.7 3.175)
		(end -3.7 -3.175)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7e99eb88-4c78-446b-bf8c-cf32a48e8765")
	)
	(fp_line
		(start -1.4 -4.175)
		(end 1.4 -4.175)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "bd1dc6e3-7dcc-47eb-80a9-bf0b5c407b73")
	)
	(fp_line
		(start -1.4 -3.175)
		(end -1.4 -4.175)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "93184e3d-7a9c-45ac-9275-b255e8e9764c")
	)
	(fp_line
		(start 1.4 -4.175)
		(end 1.4 -3.175)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9da501d4-a7b8-4b24-97f6-20454c0ffd38")
	)
	(fp_line
		(start 1.4 -3.175)
		(end 3.7 -3.175)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "c320b22e-654d-47f0-92f4-37fffb1541dc")
	)
	(fp_line
		(start 3.7 -3.175)
		(end 3.7 3.175)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9b7a1cb6-e5e1-40ba-bf03-56750ee384b9")
	)
	(fp_line
		(start 3.7 3.175)
		(end -3.7 3.175)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "be45539c-b091-4b3e-b896-2eb1aabd5e5c")
	)
	(fp_line
		(start -3.2 -2.675)
		(end 3.2 -2.675)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "266bae49-9d5c-4597-9fd3-aa1d0111c84d")
	)
	(fp_line
		(start -3.2 2.675)
		(end -3.2 -2.675)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "d0cbd4b6-a59f-4556-b15a-d7d47a7e2626")
	)
	(fp_line
		(start 3.2 -2.675)
		(end 3.2 2.675)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "208b69df-4ef5-446a-adf5-0fd462c7cf19")
	)
	(fp_line
		(start 3.2 2.675)
		(end -3.2 2.675)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "1821c262-698d-4675-b620-9653634e7e37")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "e5824777-ccde-463f-9604-3e8e6cacf6ae")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.12)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.75 -3.025)
		(size 0.3 1.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "7fb4ab58-820c-4fef-a9c7-ba79ce561e47")
	)
	(pad "2" smd roundrect
		(at -0.25 -3.025)
		(size 0.3 1.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "5725b7ce-9bb0-4952-bf23-1385ad63a963")
	)
	(pad "3" smd roundrect
		(at 0.25 -3.025)
		(size 0.3 1.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "8e39203e-22cb-4f4f-80e8-8211ae056a9a")
	)
	(pad "4" smd roundrect
		(at 0.75 -3.025)
		(size 0.3 1.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "d2cc08bf-6eec-47a1-8459-53c3816b8a7e")
	)
	(pad "MP" smd rect
		(at -2.45 -0.345)
		(size 2 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "962ce400-7c45-426c-ae06-41e7dd005e31")
	)
	(pad "MP" smd rect
		(at 2.45 -0.345)
		(size 2 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "c3513d95-c1b9-40fb-a55c-8778438d768c")
	)
)
